{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Tabelle1","Tabelle2"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":16,"n_cols":14,"rows_kept":16,"cut":false,"hidden":false,"merged":[[15,6,15,7],[11,9,11,12],[13,8,13,10],[13,6,13,7],[14,6,14,7]]}
["Messprotokoll zur elektrischen Prüfung des PV-Generators gemäß DIN EN 62446 (VDE 126-23)"]
[]
["PV-Anlage:","BENNING GmbH & Co. KG",null,null,"Prüffirma:","BENNING Service",null,null,null,"Logo:"]
[null,"Münsterstrasse 135-137",null,null,null,"Robert-Bosch-Str. 20"]
[null,"46397 Bocholt",null,null,null,"46397 Bocholt"]
[null,"Tel: 02871/930",null,null,null,"Tel: 02871/93-555"]
["Kontakt:","Herr Mustermann",null,null,"Prüfer:","Herr Mustermann"]
["Grund der Prüfung: ",null,"Erstprüfung",null,"Wiederholungsprüfung",null,"Änderung",null,"Instandsetzung","Datum:",null,"Protokoll Nr.:"]
["Beschreibung der PV-Anlage:",null,null,null,null,null,null,null,null,null,null,null,null,"Hinweis zum Datenimport:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"1. PV 1-1 oder PV 2 Datenimport durchführen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Falls zum SUN 2 keine Funkanbindung bestand:"]
[null,null,null,null,null,null,null,null,null,"Hier klicken um CSV-Datei zu importieren!",null,null,null,"2. SUN 2 Datenimport durchführen"]
["Verwendete Prüfgeräte:",null,null,null,null,null,null,null,null,null,null,null,null,"Zuordnung erfolgt anhand Datum-/Zeitstempel."]
["BENNING PV 1-1/PV 2:",null,null,null,null,null,"BENNING CC 3",null,"BENNING SUN 2",null,null,"Prüfung vom …"]
[null,null,null,null,null,null,"Serial no:",null,"Serial no:"]
["Strang","Schutzleiter-widerstand","Leerlauf-spannung","Kurzschluss-strom","Isolations-widerstand","Prüf-spannung","DC-Strangstrom oder     AC-Strom",null,"Bestrahlungs-stärke","Luft-temper.","PV-Modul-temperatur","Uhrzeit","Datum"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}